October 9, 2025
Planning and Implementation Technical Team Recommendation:
“The Planning and Implementation (PI) Technical Team recommends to the U.S. Department of the Interior to implement a fall High-Flow Experiment (HFE) at 33,000 CFS for 27 hours as described in the attached Tech Team Report.”
Considerations:
· At this time Grand Canyon Monitoring and Research Center (GCMRC) has been unable to provide a secondary review of the technical report. The Technical Team recommends that the GCMRC scientists provide a final review of the technical memo when they return to work and report any red flags to the Technical Team prior to initiating the experiment. Additionally, the fall HFE under consideration is limited in magnitude and duration and could provide a valuable learning opportunity for potential future hydrological scenarios. If new evidence is found that a smallmouth bass spawn occurred in the summer of 2025, the possibility that a fall HFE could disperse those small fish downstream should be evaluated. This recommendation is based on the understanding by the technical team that conducting a fall HFE will not impact the resources or scientific integrity of a potential Cool Mix Flow in 2026. 
· Monitoring of the fall HFE will include remote sensing and camera analyses. If staffing is available, physical sandbar monitoring is suggested to evaluate the impacts of this fall HFE.
· We encourage continued communication as things develop around the fall HFE. 
